From 11dc456aeb21659c668e3d244046ecbd0322b79d Mon Sep 17 00:00:00 2001
From: Aleksa Vučković <aleksav013@gmail.com>
Date: Sun, 29 May 2022 01:06:17 +0200
Subject: MBR

---
 kernel.tex | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

(limited to 'kernel.tex')

diff --git a/kernel.tex b/kernel.tex
index 409818f..9778ac7 100644
--- a/kernel.tex
+++ b/kernel.tex
@@ -495,6 +495,22 @@ Taj program se naziva {\eng Bootloader}.
 
 %{\eng\url{https://wiki.osdev.org/Boot_Sequence}}
 
+\section{{\eng MBR}}
+\medskip
+
+{\eng MBR (Master Boot Record)} je prvi sektor na hard disku. Sadrzhi {\eng
+bootloader} i tabelu particija. Od 512 bajtova koje chini sektor hard diska,
+440-446 bajtova je predvidjeno za {\eng bootloader}, 64 bajta za 4 primarne
+particije dok poslednja dva bajta sadrzhe konstante {\eng 0x55, 0xAA} koje
+identifikuju ovaj sektor kao validan {\eng boot} sektor.\\
+
+Noviji {\eng UEFI (Unified Extensible Firmware Interface)} sistemi umesto {\eng
+MBR} sadrzhe {\eng GPT (GUID partition table)} tabelu particija. {\eng UEFI}
+omoguc1ava particionisanje hard diskova vec1ih od {\eng 2TB}, kao i posedovanje
+vishe od 4 primarne particije.
+
+\newpage
+
 \section{{\eng Bootloader}}
 \medskip
 
-- 
cgit v1.2.3

